**Draft Drainage 2019/20 Capital Programme**

| **Programme: Drainage** | | | | |
| --- | --- | --- | --- | --- |
| **Project Name/Location** | **Division** | **District** | **Project Description** | **Estimate** |
| **Countywide Capital Allocation:** | | | | **£1,000,000** |
| 19/20 B6254 Kirkby Lonsdale Road, Arkholme | Lancaster Rural North | Lancaster | Upsize the culvert from 100mm to 150mm downhill from the Forge, Snab Green Lane | £25,000 |
| 19/20 Morecambe Road/school watercourses | Morecambe South & Skerton | Lancaster | Clean out dykes and survey of drain under Hadrians Road | £15,000 |
| 19/20 A6068 Padiham Barrowford bypass | Pendle Hill | Pendle | Upgrade drainage and culvert repairs | £28,000 |
| 19/20 Ash Lane brick culvert phase 2 | Fylde East | Fylde | Construction of phase 2 | £75,000 |
| 19/20 A59 Preston New Road, Samlesbury | South Ribble East | South Ribble | Upsize 7 carriageway gullies on hill above former police houses to catch volume of surface water and reduce ponding in front of residential property | £15,000 |
| 19/20 New Cut Lane, Halsall | West Lancashire West | West Lancs | Drainage investigation, and renew surface water drain in highway | £35,000 |
| 19/20 A588 Marsh Lane, Cockerham | Lancaster Central | Lancaster | Drainage carriageway and footway works to install non-return valves at private connections, and increase drainage pipe capacity | £50,000 |
| 19/20 C278 Chain Lane, Staining phase 1 | Fylde West | Fylde | Repair and improve capacity of highway drainage system at roundabout, including repairs to damaged 3rd party assets | £80,000 |
| 19/20 Hall Lane, Appley Bridge | Skelmersdale East | West Lancs | Rebuild culvert headwall | £20,000 |
| 19/20 Higher Lane, Dalton near Brookside | West Lancashire East | West Lancs | Replace culvert | £20,000 |
| 19/20 Asmall Lane, Halsall | West Lancashire West | West Lancs | Install 300m of new 300mm diameter pipe and manholes | £52,000 |
| 19/20 Towneley Close, Lancaster City | Lancaster Central | Lancaster | Additional gullies and capacity to reduce risk of flooding | £50,000 |
| 19/20 Redgate, Ormskirk | Ormskirk | West Lancs | Replace culvert under the highway (from ginnel to back of No 36) | £30,000 |
| 19/20 Sandy Lane, Accrington Phase 2 - option appraisal | Accrington South | Hyndburn | Review options identified in phase 1 | £10,000 |
| 19/20 Footpath 2 Barrow Lane/ Hexham Road, Torrisholme | Morecambe South | Lancaster | Install debris trap/s to allow for cleaning and reduce risks of gravel reaching highway drainage systems | £20,000 |
| 19/20 Hatlex Lane, Hest Bank | Morecambe North | Lancaster | Install gullies and carrier drain, with 5 pairs of gullies | £50,000 |
| 19/20 Edge End Avenue, Brierfield (rear of 21 - 27) Phase 2 | Pendle Hill | Pendle | Complete works to locate culverted watercourse under footpath and back gardens. Repair any damage and clear outfall to highway drainage | £30,000 |
| 19/20 Red Cat Lane, Burscough | Burscough and Rufford | West Lancs | Install 140m of new 300mm diameter pipe and manholes | £30,000 |
| 19/20 Lancaster Road, Overton | Heysham | Lancaster | Continuing investigation into drainage system | £15,000 |
| 19/20 Brookhouse/Caton | Lancaster Rural East | Lancaster | Investigation of current highway system | £10,000 |
| 19/29 Priest Hutton highway drainage improvements | Lancaster Rural North | Lancaster | Highway drainage improvements | £15,000 |
| 19/20 A6 Hampson Road junction | Lancaster Rural East | Lancaster | Culvert damage assessment and options review | £10,000 |
| 19/20 A683 Denny Beck to Scarthwaite Bends | Lancaster Rural East | Lancaster | Clean system and check for faults | £6,000 |
| 19/20 A6 Milnthorpe Road | Lancaster Rural North | Lancaster | De-silting of drainage system and pipe work repairs | £25,000 |
| 19/20 A6 Scotforth Road | Lancaster Central, Lancaster South East, Lancaster Rural East | Lancaster | De-silting of the carrier drain | £25,000 |
| 19/20 Abbeystead Lane Cattle grid to Abbeystead Road | Lancaster Rural East | Lancaster | Clean system and check for faults | £6,000 |
| 19/20 Burnley Road, Hapton | Padiham and Burnley West | Burnley | Drain survey and lay new drainage | £12,000 |
| 19/20 Carr Lane, Middleton | Heysham | Lancaster | Review drainage system | £15,000 |
| 19/20 Moor Lane Wray Curwen Hall Farm | Lancaster Rural East | Lancaster | Relay drain and check outfalls | £10,000 |
| 19/20 Crown Point Road between 385350 and Burnley Road | Burnley Rural | Burnley | Lay 145m of 150mm pipe, and 4 gullies | £36,000 |
| 19/20 Castle Lane, Ormskirk | West Lancashire East | West Lancs | Install 270m of new 225mm diameter pipe and manholes | £45,000 |
| 19/20 Sawley Old Brow Phase 2 | Ribble Valley North East | Ribble Valley | Relocate private septic tank discharge to United Utilities foul sewer | £10,000 |
| 19/20 New Road Silverdale before Sand Pool | Lancaster Rural North | Lancaster | Culvert collapse repairs | £15,000 |
| 19/20 Ravensclose Road, Wennington Ravens Close Farm | Lancaster Rural East | Lancaster | Install new gullies and drain | £15,000 |
| 19/20 Moor Lane Wray, Curwen Hall Farm | Lancaster Rural East | Lancaster | Relay drain and check outfalls | £10,000 |
| 19/20 C332 Pedders Lane junction with Whinfield Lane | Preston South West | Preston | Works in 2 locations (at junction, and approx 50m north on Pedders Lane): Investigation, design and corrective measures to redirect water off the highway | £15,000 |
| 19/20 Storrs Lane, Silverdale | Lancaster Rural North | Lancaster | Investigate culvert as possible collapse | £15,000 |
| 19/20 Gincroft Lane, Edenfield | Rossendale South | Rossendale | Ground water seeping through carriageway. Install new interception drain and channels | £20,000 |
| 19/20 Clod Lane, Haslingden | Rossendale South | Rossendale | Ground water eroding edge of carriageway. Improve existing drainage system and install channels | £35,000 |
| **Forecast Outturn Capital Expenditure:** | | | | **£1,000,000** |